| TIBURON(GK) >2005 > G 2.7 DOHC > Emission Control System > Evaporative Emission Control System > Purge Control Solenoid Valve (PCSV)>Repair procedures |

INSPECTION
When disconnecting the vacuum hose, make an identification mark on it so that it can be reconnected to its original position.
1. | Disconnect the vacuum hose from the solenoid valve.
2. | Detach the harness connector.
3. | Connect a vacuum pump to the nipple to which the red-striped vacuum hose was connected.
4. | Apply vacuum and check when voltage is applied to the PCSV and when the voltage is discontinued.
Battery voltage | Normal condition
When applied | Vacuum is released
When discontinued | Vacuum is maintained
5. | Measure the resistance between the terminals of the solenoid valve.
PCSV coil resistance (Ω): 24.5 ~ 27.5 Ω at 20°C (68°F)