| TIBURON(GK) >2005 > G 2.7 DOHC > Body Electrical System > Windshield Wiper/Washer > Front Wiper Motor>Repair procedures |

REMOVAL
1. | Remove the wiper arm.
Care must be taken not to scratch the engine hood.
Tightening torque 23~28 Nm (230~280 kg•cm, 16.9~20.6 lb•ft)
2. | Remove the weatherstrip and cowl top cover after removing the retainers.
3. | Disconnect the windshield wiper motor connector and remove the 3 bolts holding the windshield wiper motor and linkage assembly.
Tightening torque 7~11 Nm (70~110 kg•cm, 5.1~8.0 lb•ft)
4. | Installation is the reverse of removal.
INSTALLATION
1. | Install the wiper arm to the specified position.
Specified position | A | B
Distance (mm) | 30~40 | 30~40
2. | Set the washer nozzle on the specified spray position.
INSPECTION
SPEED OPERATION CHECK
1. | Remove the connector from the wiper motor.
2. | Attach the positive (+) lead from the battery to terminal 3 and the negative (-) lead to terminal 4.
3. | Check that the motor operates at low speed.
4. | Connect the positive (+) lead from the battery to terminal 3 and the negative (-) lead to terminal 5.
5. | Check that the motor operates at high speed.
AUTOMATIC STOP OPERATION CHECK
1. | Operate the motor at low speed using the stalk control.
2. | Stop the motor operation anywhere except at the off position by disconnecting terminal 4.
3. | Connect terminals 2 and 4.
4. | Connect the positive (+) lead from the battery to terminal 3 and the negative (-) lead to terminal 1.
5. | Check that the motor stops running at the off position.