| TIBURON(GK) >2005 > G 2.7 DOHC > Body Electrical System > Daytime Running Lights > DRL Control Module>Repair procedures |

INSPECTION
OPERATION CHECK INSPECT CIRCUITS FOR DAYTIME RUNNING LIGHT SYSTEM
1. | Disconnect the wire connector to DRL module from engine compartment.
2. | Inspect the connector on wire harness side as shown.
Check For | Test Connect | Condition | Test Specification
Continuity | 4-Ground | Parking brake switch | OFF (Released) | No continuity
ON (Pull up) | Continuity
5-Ground | Head lamp switch | OFF | No continuity
ON | Continuity
6-Ground | Constant | Continuity
9-Ground | Dimmer&passing switch | Head light ON | Continuity
Head light OFF | No continuity
Voltage | 9-Ground | Ignition switch | ON | Battery voltage
ACC or LOCK | No voltage
5-Ground | Ignition switch | ON | Battery voltage
ACC or LOCK | No voltage
7-Ground | Constant | Battery voltage
3-Ground | Engine | Stop | No voltage
Running | Battery voltag
3. | If circuit is not as specified, refer to schematic diagram and inspect for short circuits.