| TIBURON(GK) >2005 > G 2.7 DOHC > Heating,Ventilation, Air Conditioning > Heater > Mode Control Actuator>Description and Operation |

DESCRIPTION
- | Operating temp. : -30°C ~ +80°C
- | Operating voltage : DC 9V ~ 16V
- | Rated voltage : DC 12V
- | Rated load : 4kgf/cm
- | Rated voltage : DC 12V
- | Rated watt. : 0.25W (at 40°C)
- | Opration volt : DC 5V ± 0.5V
- | Total resistance : 5kΩ ± 10%
- | Output lock torque : Min 1.76Nm (18kgf/cm) (at DC 12V)
- | Rated AMP. : Max 150mA
- | Lock vol. : Max. 400mA
- | Characteristics