| TIBURON(GK) >2005 > G 2.7 DOHC > Body Electrical System > General Information>Specifications |

SPECIFICATIONS
MULTIFUNCTION SWITCH
Items | Specifications
Rated Voltage | DC 12V
Operating temperature range | -30°C ~ +80°C (-22 ~ +176°F)
Rated load Dimmer & passing switch Lighting switch Turn signal & lane change switch Wiper switch Wiper mist switch Washer switch Variable intermittent wiper volume switch Rear wiper & washer switch Horn switch | High : 1A (Relay load) Low : 1A (Relay load) Passing : 1A (Relay load) Lighting : 1A (Relay load) 6.6 ± 0.5A (Lamp load) Low, High : 4.5A (Motor load) Int. : 0.22 ± 0.05A (Relay load) Lock : Max. 28A (Motor load) 4.5A (Motor load) 4A (Motor load) Max. 25mA Rear wiper : 0.2A (Relay load) Rear washer : 4A (Motor load) 1A (Relay load)
INSTRUMENTS AND WARNING SYSTEM
Warning lamps | Bulb wattage (W) | Color
High beam Low fuel Turn signal (LH, RH) Battery (charge) Oil pressure Air bag Parking brake Seat belt Check engine ABS Door ajar Trunk lid open Cruise TCS TCS OFF | LED LED LED LED LED Bulb (1.4W) LED LED Bulb (1.4W) LED LED LED LED LED LED | Blue Amber Green Red Red Red Red Red Amber Amber Red Red Green Amber Amber
INDICATORS AND GAUGES
LIGHTING SYSTEM
Items | Bulb wattage (W)
Head lamp | 55W / 55W (High / Low beam)
Front turn signal/position lamp | 28W / 8W
Front position lamp | 5W
Front fog lamp | 51W
Rear combination lamps Tail/stop lamp Back up lamp Turn signal lamp (Front/Rear) | 8W / 27W 27W 28W/27W
Side marker lamp (Front/Rear) | 8W/5W
Luggage lamp | 5W
Center high mounted stop lamp | Internal type : 2.4W (LED) External spoiler type : 3.5W (LED)
Overhead console lamp | 10W x 2
License plate lamp | 5W x 2
AUDIO
Items | H250 | H260 | H280
Rated output | Max. 20W x 4 | Max. 20W x 4 | Max. 24W x 4
Load impedance | 4Ω x 4 | 4Ω x 4 | 4Ω x 4
Band | AM/FM | AM/FM | AM/FM
Tuning type | PLL Synthesized type | PLL Synthesized type | PLL Synthesized type
Dark current | Max. 2mA | Max. 3.8mA | Max. 2mA
Frequency range / Channel | AM : 530~1710KHZ/10KHZ | AM : 530~1710KHZ/10KHZ | AM : 530~1710KHZ/10KHZ
FM : 87.9~107.9MHZ/200KHZ | FM : 87.9~107.9MHZ/200KHZ | FM : 87.9~107.9MHZ/200KHZ
WINDSHIELD WIPER AND WASHER
Items | Specifications
Wiper motor Rated voltage Operating voltage range Insulation resistance Speed/current at 1Nm load test Speed/current at 4Nm load test Torque/current when parking | DC 12V DC 10~15V Min. 1MΩ Low : 44~52 rpm / 3.5A or less High : 64~78 rpm / 4.5A or less Low : 39~47 rpm / 5.5A or less High : 56~68 rpm / 7.0A or less Low : 28Nm / 24A or less High : 23Nm / 28A or less
Windshield washer Motor type Pump type Rated voltage Discharge pressure Flow rate Current Overload capacity (Continuous operation) With water Without water (Racing) | DC ferrite magnet Centrifugal 12V 1.8kg/cm² or more 1,450cc/min. or more 5.0A or less 60sec. or less 20sec. or less
Rear wiper motor Speed/current at no load test Speed/current at 1Nm load test Torque/current when parking Wiping angle at no load | 35rpm/2.2A or less 30~40rpm/3.5A or less 8Nm/14A or less 170° ± 3°