| TIBURON(GK) >2005 > G 2.7 DOHC > Restraint > Airbag Module > Driver Airbag (DAB) Module and Clock Spring>Repair procedures |

REMOVAL
1. | Disconnect the negative battery cable and keep secure from battery.
Wait at least 3 minutes after disconnecting the battery cable before doing any further work.
2. | Remove the side protect cover of steering wheel and airbag module mounting bolts using a hexagonal wrench.
3. | When disconnecting the connector of the clock spring from the airbag module, pull the airbag's lock toward the outer side to spread it open.
When disconnecting the airbag module-clock spring connector, take care not to apply excessive force to it.
4. | Remove the drive airbag module.
The removed airbag module should be stored in a clean, dry place with the pad cover face up.
5. | Remove the steering wheel using SST (09561-11002).
Do not hammer on the steering wheel. Doing so may damage the collapsible column mechanism.
INSPECTION
AIRBAG MODULE Dispose the old one according to the specified procedure.
Never attempt to measure the circuit resistance of the airbag module (squib) even if you are using the specified tester. If the circuit resistance is measured with a tester, accidental airbag deployment will result in serious personal injury.
1. | Check pad cover for dents, cracks or deformities.
2. | Check the airbag module for denting, cracking or deformation.
3. | Check hooks and connectors for damage, terminals for deformities, and harness for binds.
4. | Check airbag inflator case for dents, cracks or deformities.
5. | Install the airbag module to the steering wheel to check for fit or alignment with the wheel.
CLOCK SPRING
1. | If, as a result of the following checks, even one abnormal point is discovered, replace the clock spring with a new one.
2. | Check connectors and protective tube for damage, and terminals for deformities.