| TIBURON(GK) >2005 > G 2.7 DOHC > Body (Interior and Exterior) > Exterior > mirror>Repair procedures |

REMOVAL AND INSTALLATION
OUTSIDE REARVIEW MIRROR
1. | Remove the outside rearview mirror cover.
2. | Loosen the mounting bolts, disconnet the connector and then remove the outside rearview mirror.
Tightening torque: 6.9~10.8 N•m (0.7~1.1 kgf•m, 5.1~8.0 lbf•ft)
3. | Installation is the reverse of removal.
INSIDE REARVIEW MIRROR
1. | Remove the rearview mirror.
2. | Installation is the reverse of removal.
DISASSEMBLY
Wear gloves to remove and install the mirror holder.
1. | Insert a flat tip screwdriver between the outside rear view mirror holder and mirror assembly.
When prying with a flat tip screwdriver, wrap it with a shop towel to prevent damage.
2. | Remove the outside rear view mirror actuator from outside rear view mirror housing.
3. | Installation is the reverse of removal.