| TIBURON(GK) >2006 > G 2.0 DOHC > Restraint > Supplemental Restraint System Control Module (SRnodeM) > SRS Control Module (SRnodeM)>Repair procedures |

REMOVAL
1. | Disconnect the battery negative cable, and wait at least 3 minutes before begining work.
2. | Disconnect the airbag connectors.
3. | Remove the center console. (Refer to BD group).
4. | Disconnect the connector from the SRS unit.
5. | Remove the three bolts from the SRS unit, then pull out the SRS unit from the bracket.