| TIBURON(GK) >2006 > G 2.0 DOHC > Fuel System > Fuel Delivery System > Fuel Pump>Repair procedures |

REMOVAL (INCLUDING FUEL FILTER AND FUEL PRESSURE REGULATOR)
1. | Remove the rear seat cushion (Refer to "BD" group in this SHOP MANUAL).
2. | Open the service cover (A) under the rear seat cushion.
3. | Release the internal pressure of the fuel lines and hoses as following:
A. | Disconnect the fuel pump assembly harness connector (A).
B. | Start the engine and wait until fuel in fuel line is exhausted. After the engine stalls, turn the ignition switch to OFF position.
C. | Disconnect the negative (-) terminal from the battery.
4. | Disconnect the fuel feed line (B) and suction hose(C).
Cover the hose connection with a shop towel to prevent splashing of fuel caused by residual pressure in the fuel line
5. | Unfasten the fuel pump assembly mounting bolts (D).
6. | Remove the fuel pump assembly.