| TIBURON(GK) >2006 > G 2.0 DOHC > Engine Electrical System > General Information>Specifications |

SPECIFICATION
IGNITION SYSTEM
Items | Specifications
2.0 | 2.7
Ignition coil | Type | Mold coil type
Primary resistance | 0.58 ± 10% (Ω) | 0.74 ± 10% (Ω)
Secondary resistance | 8.8 ± 15% (kΩ) | 13.3 ± 15% (kΩ)
Spark plugs | NGK | BKR5ES-11 | PFR5N-11
CHAMPION | RC10YC4 | RC10PYPB4
Gap | 1.0 ~ 1.1 mm (0.039 ~ 0.043 in.)
STARTING SYSTEM
Items | Specifications
2.0 | 2.7
Starter | Type | Reduction drive (with planetary gear)
Rated voltage | 12V, 1.2KW
No.of pinion teeth | 8
No-load characteristics | Voltage | 11V
Amperage | 90A, MAX
Speed | 3,000rpm, MIN | 2,800rpm, MIN
CHARGING SYSTEM
Items | Specifications
2.0 | 2.7
Generator | Type | Battery boltage sensing
Rated voltage | 13.5V, 90A | 12V, 120A
Speed in use | 1,000 ~ 18,000 rpm
Voltage regulator | Electronic built-in type
Regulator setting voltage | 14.4 ± 0.2V | 14.55 ± 0.2V
Temperature compensation | -10 ± 3mV/°C | -3.5 ± 1mV/°C
Battery | Type | MF 60 AH | MF 68 AH
Cold cranking amperage [at -18°C (0°F)] | 550A | 600A
Reserve capacity | 92min | 110min
Specific gravity [at 25°C (77°F)] | 1.280 ± 0.01 | 1.280 ± 0.01
- | COLD CRANKING AMPERAGE is the amperage a battery can deliver for 30 seconds and maintain a terminal voltage of 7.2V or greater at a specified temperature.
- | REVERSE CAPACITY RATING is the amount of time a battery can deliver 25A and maintain a minimum terminal voltage of 10.5V at 26.7°C(80°F)
AUTO CRUISE CONTROL SYSTEM
Items | Specification
Setting error | Within ± 1.5Km/h on level road (± 1MPH)
Vehicle speed memory variation | No variation
Setting time | 0.1sec max.
Resuming time | 0.1sec max.
Minimum operating speed | 40 ± 2Km/h (25 ± 1.2MPH)
Cancel speed range | 15 ± 2Km/h (9 ± 1.2MPH)
Maximum memorized speed | 160 ± 2Km/h (99 ± 1.2MPH)
Pulling force | 127N(13Kgf)(28.6 Ib-force)
Main switch serial resistance value | 3.9kΩ ± 1%
Command switch serial resistance value | SET switch : 220Ω ± 1%
RESUME switch : 910Ω ± 1%
TIGHTENING TORQUE
Items | Nm | kg•cm | lb•ft
Generator terminal (B+) Starter motor terminal (B+) Battery terminal Spark plug | 5 ~ 7 10 ~ 12 4 ~ 6 20 ~ 30 | 50 ~ 70 100 ~ 120 40 ~ 60 200 ~ 300 | 3.6 ~ 5.1 7.3 ~ 8.8 2.9 ~ 4.3 15 ~ 22