| TIBURON(GK) >2006 > G 2.0 DOHC > Body (Interior and Exterior) > General Information>Specifications |

SPECIFICATIONS
Hood
- | Type
| Rear hinged, front opening type (gaslifter type)
Door
- | Construction
- | Regulator system
- | Locking system
| Front hinged, full door construction Wire drum type Pin-fork system
Tailgate
- | Type
| Inner hinged, gas lifter type
Glass thickness mm(in.)
- | Windshield glass
- | Door glass
- | Quarter fixed glass
- | Tailgate glass
| 5 (0.20) 5 (0.20) 3.2 (0.13) 3.5 (0.14)
Seat belt | 3 point type with E.L.R
E.L.R. : Emergency Locking Retractor
TIGHTENING TORQUE
| N•m | Kgf•m | lbf•ft
Door
- | Door hinge to body
- | Door hinge to door
- | Door striker mounting bolt
| 34.3~41.2 9.8~11.8 16.7~21.6 | 3.5~4.2 1.0~1.2 1.7~2.2 | 25.3~30.4 7.2~8.7 12.3~15.9
Tailgate
- | Tailgate hinge to body
- | Tailgate hinge to tailgate
- | Tailgate latch mounting bolt
- | Tailgate striker mounting bolt
| 21.6~26.5 6.9~8.8 6.9~8.8 8.8~13.7 | 2.2~2.7 0.7~0.9 0.7~1.1 0.9~1.4 | 15.9~19.5 5.1~6.5 5.1~8.0 6.5~10.1
Hood
- | Hood hinge to body
- | Hood hinge to hood
- | Hood latch to body
- | Gas lifter mounting bolt
| 21.6~26.5 21.6~26.5 6.9~10.8 8.8~13.7 | 2.2~2.7 2.2~2.7 0.7~1.1 0.9~1.4 | 15.9~19.5 15.9~19.5 5.1~8.0 6.5~10.1
Seat
- | Front seat to floor, Bolt
- | Rear seat back center bracket, Bolt
- | Rear seat back lower side bracket, Bolt
- | Rear seat cushion mounting, Bolt
| 34.3~53.9 16.7~25.5 16.7~25.5 16.7~25.5 | 3.5~5.5 1.7~2.6 1.7~2.6 1.7~2.6 | 25.3~39.8 12.3~13.7 12.3~13.7 12.3~13.7
Seat belt
- | Front seat belt retractor mounting bolt
- | Front seat belt upper anchor mounting bolt
- | Front seat belt sliding bar mounting bolt
- | Front seat belt height adjuster mounting bolt
- | Rear seat belt retractor mounting bolt
- | Rear seat belt upper anchor mounting bolt
- | Front seat belt buckle mounting bolt
| 39.2~53.9 39.2~53.9 39.2~53.9 39.2~53.9 39.2~53.9 39.2~53.9 39.2~53.9 | 4.0~5.5 4.0~5.5 4.0~5.5 4.0~5.5 4.0~5.5 4.0~5.5 4.0~5.5 | 28.9~39.8 28.9~39.8 28.9~39.8 28.9~39.8 28.9~39.8 28.9~39.8 28.9~39.8
Sunroof
- | Sunroof lid panel mounting, Nut
- | Sunroof assembly mounting, Bolt
| 6.9~8.8 6.9~10.8 | 0.7~0.9 0.7~1.1 | 5.1~6.5 5.1~8.0