| TIBURON(GK) >2006 > G 2.0 DOHC > Engine Electrical System > Cruise Control System > Cruise Control Cable>Repair procedures |

Removal
1. | Disconnect the battery negative (-) cable.
2. | Remove the auto cruise cable adjustment clip (A).
3. | Remove the auto cruise cable retaining grommet (B) from the bracket.
4. | Manually open the throttle body to the Wide Open throttle (W.O.T) position and disconnect the throttle cable from the throttle lever.
Damage to the auto cruise cable or the accelerator cable may result if the throttle lever is rotated by lifting up on the cable. When connecting the auto cruise cable from the throttle lever, rotate the throttle lever only by lifting up on the lever itself.
Installation
1. | Install the cruise control actuator. (Refer to Cruise Control System - Cruise Control Actuator)
2. | Manually open the throttle body to the Wide Open throttle (W.O.T) position and connect the throttle cable from the throttle lever.
Damage to the auto cruise cable or the accelerator cable may result if the throttle lever is rotated by lifting up on the cable. When connecting the auto cruise cable from the throttle lever, rotate the throttle lever only by lifting up on the lever itself.
3. | Install the auto cruise cable retaining grommet (B) from the bracket.
4. | Install the auto cruise cable adjustment clip (A) after adjusting the cable to the position just before rotating the throttle lever.
When installing the auto cruise cable to the throttle lever, be careful not to bend or twist the cable. Check the cable and hose routings to ensure that they do not interfere with the throttle body, accelerator cable and etc..
5. | Disconnect the battery negative (-) cable.