| TIBURON(GK) >2006 > G 2.0 DOHC > Clutch System > Clutch System > The Other Clutch System Component>Repair procedures |

SERVICE ADJUSTMENT PROCEDURE
CLUTCH PEDAL INSPECTION AND ADJUSTMENT
1. | Measure the clutch pedal height (from the face of the pedal pad to the floorboard) and the clutch pedal clevis pin play (measured at the face of the pedal pad).
(A) 166.9 mm
2. | If the clutch pedal clevis pin free-play is not within the standard value range, adjust as follows:
A. | Turn and adjust the bolt, then secure by tightening the lock nut.
After the adjustment, tighten the bolt until it reaches the pedal stopper, and then tighten the lock nut.
• | Turn the push rod to agree with the standard value and then secure the push rod with the lock nut.
When adjusting the clutch pedal height or the clutch pedal clevis pin play, be careful not to push the push rod towardthe master cylinder.
3. | After completing the adjustments, check that the clutch pedal free play (measured at the face of the pedal pad) is within the standard value ranges.
Standard value: (B) 6~13 mm (0.24~0.52 in.) (C) 50 mm (1.5 in.)
4. | If the clutch pedal free play, and the distance between the clutch pedal and the floor board when the clutch is disengaged, do not meet with the standard values, it may be the result of either air in the hydraulic system or a faulty clutch master cylinder. Bleed the air or disassemble and inspect the master cylinder or clutch.
BLEEDING
Use the specified fluid. Avoid mixing different brands of fluid.
SAE J1703 (DOT 3 or DOT 4)
1. | Loosen the bleeder screw at the clutch release cylinder.
2. | Push the clutch pedal down slowly until all is expelled.
3. | Hold the clutch pedal down until the bleeder is retightened.
4. | Refill the clutch master cylinder with the specified fluid.
The rapidly-repeated operation of the clutch pedal in B-C range may cause the release cylinder's position to be forcedout from the release cylinder body during air bleeding, Repress the clutch pedal after it returns to the "A" point completely.