| TIBURON(GK) >2006 > G 2.0 DOHC > Body Electrical System > Rear Wiper/Washer > Rear Washer Motor>Repair procedures |

INSPECTION
1. | With the washer motor connected to the reservoir tank, fill the reservoir tank with water.
2. | Connect positive(+) and negative(-) battery cables to terminals 3 and 1 respectively to see that the washer motor runs and water is pumped.
3. | Check that the motor operates normally. Replace the motor if it operates abnormally.