| TIBURON(GK) >2006 > G 2.0 DOHC > Emission Control System > General Information>Specifications |

SPECIFICATIONS
Item | Specification
Purge Control Solenoid Valve (PCSV) | Type | Duty Control type
Resistance (Ω) | 24.5 ~ 27.5 at 20 °C (68 °F)
Canister Close Valve (CCV) | Type | ON/OFF Control type
Resistance (Ω) | 23.9 ~ 26.9 Ω at 20°C (68°F)
TIGHTENING TORQUES
Item | N•m | kgf•cm | lbf•ft
Positive Crankcase Ventilation Valve | 7.8 ~ 11.8 | 0.8 ~ 1.2 | 5.8 ~ 8.7