| TIBURON(GK) >2006 > G 2.0 DOHC > Body (Interior and Exterior) > General Information>Troubleshooting |

TROUBLESHOOTING
Trouble symptom | Probable cause | Remedy
Water leaks from sunroof | Dirt accumulated in drain tube | Clear dirt inside of drain
Clogged drain tube | Blow air into drain to remove dirt
Broken or dislocated drain tube, defective or cracked clip | Check tube installation and flange contact
Deteriorated roof lid weatherstrip | Replace
Excessive roof lid-to-body clearance and improperly fitted weatherstrip | Adjust
Wind noise around sunroof | Loose or deformed deflector, gaps in body work | Retighten adjust or replace
Sunroof makes a noise when moved | Foreign particles lodged in guide rail | Check drive cable and guide rails for foreign particles
Loose guide rails and lid | Retighten
Motor runs but sunroof does not move or moves only halfway | Foreign particles lodged in guide rail | Check drive cable and guide rails for foreign particles
Incorrect engagement of motor pinion with drive cable | Check for loose motor installation and damaged pinion
Decrease in motor's clutch slipping force | Adjust
Increased sunroof sliding resistance or interference of sunroof with drive cables, weatherstrip, etc. due to maladjustment of sunroof | Adjust or replace
Noise in motor (clutch slipping noise from motor when sunroof is fully opened or closed is not an unusual noise.) | Incorrect engagement of motor pinion with drive cable | Check pinion installation and retighten motor
Worn out or damaged motor pinion bearing | Replace motor assembly
Worn out or deformed drive cable | Replace
Door glass fails to operate up and down | Incorrect window glass installation | Adjust position
Damaged or faulty regulator arm or regulator | Correct or replace
Door does not open or close completely | Incorrect door installation | Adjust position
Defective door check assembly | Correct or replace
Door hinge requires grease | Apply grease
Hood does not open or close completely | Striker and latch not properly aligned | Adjust
Incorrectly installed hood | Adjust
Incorrect hood bumper height | Adjust
Water leak through windshield and rear window | Defective seal | Fill with sealant
Defective flange | Correct
Wind noise around door | Weatherstrip not holding firmly | Adjust fit of door
Improperly installed weatherstrip | Repair or replace
Improperly closed door | Adjust
Improperly fit door | Adjust
Improper clearance between door glass and division channel | Adjust
Deformed door | Repair or replace