| TIBURON(GK) >2006 > G 2.0 DOHC > Clutch System > General Information>Specifications |

SPECIFICATIONS
Clutch operating method | Hydraulic type
Clutch disc
- | Type
- | Facing diameter (Outside x Inside) mm (in.)
| Single dry with diaphragm. 215 x 145 (8.5 x 5.7)
Clutch cover assembly
- | Type
| Diaphragm spring strap
Clutch release cylinder * I.D. mm (in.) | 2.0L : 19.05 (0.76) 2.7L : 20.64 (0.82)
Clutch master cylinder * I.D. mm (in.) | 15.87(0.62)
* I.D. : Inside Diameter
SERVICE STANDARD
Clutch pedal free play | 6~13 mm (0.24~0.52 in.)
Clutch pedal height | 166.9 mm (6.676 in.)
Clutch pedal stroke | 2.0L : 145 mm (5.7 in.) 2.7L : 152 mm (6.1 in.)
Limit Clutch disc rivet sink Diaphragm spring end height difference Clutch release cylinder clearance to piston Clutch master cylinder clearance to piston | 1.1 mm (0.044 in.) 0.5 mm (0.02 in.) 0.15 mm (0.006 in.) 0.15 mm (0.006 in.)
TIGHTENING TORQUE
Item | Nm | kgf•cm | lbf•ft
Clutch pedal to pedal support member (Clutch pedal bracket) | 19~28 | 190~280 | 14~20
Clutch pedal support member to master cylinder | 8~10 | 80~100 | 6~7
Clutch tube flare nut | 13~17 | 130~170 | 9~13
Clutch tube bracket | 4~6 | 40~60 | 3~4
Reservoir band | 13~17 | 130~170 | 9~13
Clutch release cylinder | 15~22 | 150~220 | 11~16
Clutch release cylinder union bolt | 20~25 | 200~250 | 15~18
Clutch cover assembly Single mass flywheel Dual mass flywheel | 15~22 20~27 | 150~220 200~270 | 11~16 14~19
LUBRICANTS
Items | Specified lubricants | Quantity
Contact surface of release bearing and fulcrum of clutch release fork | CASMOLY L 9508 | As required
Inner surface of clutch release bearing | CASMOLY L 9508 | As required
Inner surface of clutch release cylinder and outer circumference of piston and cup | Brake fluid DOT 3 or DOT 4 | As required
Inner surface of clutch disc spline | CASMOLY L 9508 | As required
Inner surface of clutch master cylinder and outer circumference of piston assembly | Brake fluid DOT 3 or DOT 4 | As required
Clutch master cylinder push rod, clevis pin and washer | Wheel bearing grease SAE J310a, NLGI No.2 | As required
Clutch pedal shaft and bushings | SAE J310a, Chassis grease, NLGI-No.1 | As required
Contact portion of release fork to release cylinder push rod | CASMOLY L 9508 | As required
Input shaft spline | CASMOLY L 9508 | As required
Clutch release fork shaft contact portion & bushings | CASMOLY L 9508 | About lg.