| TIBURON(GK) >2006 > G 2.0 DOHC > Fuel System > General Information>Specifications |

SPECIFICATIONS
FUEL DELIVERY SYSTEM
Items | Specification
Fuel Tank | Capacity | 55 lit. (14.5 U.S.gal., 12.1 Imp. gal.)
Fuel Retrun System | Type | Returnless
Fuel Filter | Type | High pressure type (built in Fuel Pump Assembly)
Fuel Pressure Regulator | Type | Built in fuel pump assembly
Regulated Fuel Pressure | 350 kpa (3.5 kg/cm2, 49.8 psi)
Fuel Pump | Type | Electrical, in-tank type
INPUT SENSORS ▶ Type: Hot film type ▶ Specification
Test Condition | MAFS Output Voltage (V)
Idle | 0 ~ 2.0V
3000 rpm | 1.0~4.5V
Throttle Position Sensor (TPS) ▶ Type: Variable resistor type ▶ Specification
Test Condition | Signal Voltage (V) | Throttle Angle (°)
C.T | 0.2 ~ 0.8 | 0 ~ 0.5
W.O.T | 4.3 ~ 4.8 | 86
Test Condition | Resistance (kΩ) (Terminal 1 and 2) | Resistance (kΩ) (Terminal 2 and 3)
C.T | 0.71 ~ 1.38 kΩ at all temperature | 1.6 ~ 2.4 kΩ at all throttle position
W.O.T | 2.7 kΩ at all temperature
▶ Type: Zirconia Sensor ▶ Specificiation
- | Output Voltage: 0 ~ 1 V
Temperature °C (°F) | Heater Resistance (Ω)
Front HO2S | Rear HO2S
20 (68) | 9.2 | 9.2
100 (212) | 10.7 | 10.7
200 (392) | 13.1 | 13.1
300 (572) | 14.6 | 14.6
400 (752) | 17.7 | 17.7
500 (932) | 19.2 | 19.2
600 (1112) | 20.7 | 20.7
700 (1292) | 22.5 | 22.5
▶ Type: Thermistor type (built in MAFS) ▶ Specificiation
Temperature °C (°F) | Sensor Resistance (kΩ)
-20 (-4) | 14.26 ~ 16.02
0 (32) | 5.50 ~ 6.05
20 (68) | 2.35 ~ 2.54
40 (104) | 1.11 ~ 1.19
60 (140) | 0.57 ~ 0.60
80 (176) | 0.31 ~ 0.32
▶ Type: Thermistor type ▶ Specificiation
Temperature °C (°F) | Sensor Resistance (kΩ)
-20 (-4) | 14.13 ~ 16.83
0 (32) | 5.79
20 (68) | 2.31 ~ 2.59
40 (104) | 1.15
60 (140) | 0.59
80 (176) | 0.32
▶ Type: Thermistor type ▶ Specificiation
Temperature °C (°F) | Sensor Resistance (kΩ)
-20 (-4) | 16.52
0 (32) | 6.00
20 (68) | 2.45
40 (104) | 1.11
60 (140) | 0.54
80 (176) | 0.29
▶ Type: Piezoelectric type ▶ Type: Inductive type ▶ Type: Hall Effect Sensor ▶ Output Voltage (V): 0~5 ▶ Type: Hall Effect Sensor ▶ Output Voltage (V): 0~5 ▶ Type : Piezo-Resistivity type ▶ Output Voltage : Approx. 2.5V at idle OUTPUT ACTUATORS ▶ Type: Double coil type ▶ Control Frequency: 100Hz ▶ Specificiation
Temperature °C (°F) | ISCA Resistance (Ω)
Closing Coil | Opening Coil
-20 (-4) | 12.1 ~ 13.7 | 9.2 ~ 10.8
0 (32) | 13.4 ~ 15.0 | 10.2 ~ 11.8
20 (68) | 14.5 ~ 16.1 | 11.1 ~ 12.7
40 (104) | 15.7 ~ 17.3 | 12.0 ~ 13.6
60 (140) | 16.9 ~ 18.5 | 12.9 ~ 14.5
80 (176) | 18.0 ~ 19.6 | 13.8 ~ 15.4
▶ Type : Duty Control Type ▶ Specificiation
Temperature °C (°F) | OCV Resistance (Ω)
0 (32) | 6.2 ~ 7.4
20 (68) | 6.8 ~ 8.0
40 (104) | 7.4 ~ 8.6
60 (140) | 8.0 ~ 9.2
80 (176) | 8.6 ~ 9.8
▶ Type: Electromagnetic type ▶ Number: 4 ▶ Specificiation
Temperature °C (°F) | Injector Resistance (Ω)
-20 (-4) | 12.2 ~ 12.3
0 (32) | 13.3 ~ 13.5
20 (68) | 14.4 ~ 14.6
40 (104) | 15.5 ~ 15.7
60 (140) | 16.6 ~ 16.8
80 (176) | 17.7 ~ 17.9
▶ Type: Duty Control type ▶ Specificiation
Temperature °C (°F) | PCSV Resistance (Ω)
-20 (-4) | 20 ~ 24
0 (32) | 22 ~ 26
20 (68) | 24 ~ 28
40 (104) | 25 ~ 29
60 (140) | 27 ~ 31
80 (176) | 29 ~ 33
▶ Specificiation
Temperature °C (°F) | Ignition Coil Resistance
Primary Coil (Ω) | Secondary Coil (kΩ)
-20 (-4) | 0.5 | 7.7
0 (32) | 0.54 | 8.4
20 (68) | 0.58 | 9.1
40 (104) | 0.62 | 9.8
60 (140) | 0.66 | 10.5
80 (176) | 0.71 | 11.2
▶ Type : ON/OFF Control Type ▶ Resistance : 23.9 ~ 26.9 Ω at 20°C (68°F)
TIGHTENING TORQUES
ENGINE CONTROL SYSTEM
Items | N•m | kgf•m | lbf•ft
ECM Bracket | 4 ~ 6 | 0.4 ~ 0.6 | 2.9 ~ 4.3
Heated Oxygen Sensor (HO2S, Sensor 1) | 5.0 ~ 6.0 | 5.0 ~ 6.0 | 36.2 ~ 43.4
Heated Oxygen Sensor (HO2S, Sensor 2) | 50 ~ 60 | 5.0 ~ 6.0 | 36.2 ~ 43.4
Knock Sensor | 17 ~ 27 | 1.7 ~ 2.7 | 12.3 ~ 19.5
Oil Temperature Sensor (OTS) | 20 ~ 40 | 2.0 ~ 4.0 | 14.5 ~ 28.9
Crankshaft Position Sensor (CKPS) | 4 ~ 6 | 0.4 ~ 0.6 | 2.9 ~ 4.3
CKPS target wheel installation sscrew | 9.8 ~ 11.8 | 1.0 ~ 1.2 | 7.2 ~ 8.7
Camshaft Position Sensor (CMPS) | 4 ~ 6 | 0.4 ~ 0.6 | 2.9 ~ 4.3
Engine Coolant Temperature Sensor (ECTS) | 15 ~ 20 | 1.5 ~ 2.0 | 10.8 ~ 14.5
Throttle Position Sensor (TPS) | 1.5 ~ 2.5 | 0.15 ~ 0.25 | 1.1 ~ 1.8
Delivery pipe installation | 19 ~ 28 | 1.9 ~ 2.8 | 13.7 ~ 20.3
CVVT Oil control Valve (OCV) | 9.8 ~ 11.8 | 1.0 ~ 1.2 | 7.2 ~ 8.7
FUEL DELIVERY SYSTEM
Item | N•m | kgf•m | lbf•ft
Fuel pump assembly mounting screws | 2.0~2.9 | 0.2~0.3 | 1.4~2.2
Fuel vent valve mounting | 2.0~2.9 | 0.2~0.3 | 1.4~2.2
2-way valve mounting | 2.0~2.9 | 0.2~0.3 | 1.4~2.2
SERVICE STANDARD
Basic Idle rpm (After warm up) | A/C OFF | 700±100 rpm
Ignition Timing(After warm up, at idle) | BTDC 8°±5°
SEALANTS
Engine Coolant Temperature Sensor (ECTS) assemby | LOCTITE 962T or equivalent