| TIBURON(GK) >2006 > G 2.0 DOHC > Body Electrical System > Lighting System>Repair procedures |

REPLACEMENT OF LAMPS
HEAD LAMP/TURN SIGNAL LAMP
1. | Disconnect the negative battery terminal.
2. | Remove the front bumper upper cover.
3. | Remove the head lamp and turn signal lamp mounting bolts (3EA) and remove the lamp assembly.
4. | Installation is the reverse of removal.
FRONT FOG LAMP
1. | Disconnect the negative battery terminal.
2. | Remove the turn signal lamp and head lamp assembly.
3. | Remove the front bumper cover (Refer to BD group). Disconnect the wire connector and remove the front fog lamp.
4. | Installation is the reverse of removal.
REAR COMBINATION LAMP
1. | Disconnect the negative battery terminal.
2. | Remove the luggage trim side cover.
3. | Remove the 3 screws holding the rear combination lamp and disconnect the wire connectors.
4. | Remove the rear combination lamp assembly.
5. | Installation is the reverse of removal.
CENTER HIGH MOUNTED STOP LAMP
1. | Disconnect the negative battery terminal.
2. | Remove the rear spoiler after removing 4 nuts. (External spoiler type)
3. | Remove the center high mounted stop lamp assembly.
4. | Installation is the reverse of removal.
LICENSE PLATE LAMP
1. | Disconnect the negative battery terminal.
2. | Remove the mounting screws and disconnect the lamp connector.
3. | Installation is the reverse of removal.
OVERHEAD CONSOLE LAMP
1. | Disconnect the negative battery terminal.
2. | Detach the map lamp lens from the lamp assembly with a flat-tip screwdriver.
3. | Detach the lamp assembly from the headliner after removing the 4 screws.
4. | Disconnect the wiring connectors from the headliner.
5. | Installation is the reverse of removal.
LUGGAGE LAMP
1. | Disconnect the negative battery terminal.
2. | Detach the luggage lamp assembly from the luggage side trim with a flat-tip screwdriver.
3. | Installation is the reverse of removal.
INSPECTION OF COMPONENTS
HEAD LAMP RELAY
1. | Remove the head lamp relay from the relay box in the engine compartment.
2. | Check for continuity between terminals on the relay.
HAZARD SWITCH
1. | Disconnect the negative (-) battery terminal.
2. | Remove the center facia panel with a flat-tip screwdriver.
3. | Detach the hazard lamp switch from the center facia panel.
4. | Operate the switch and check for continuity between terminals with an ohmmeter.
RHEOSTAT
1. | Disconnect the negative (-) battery terminal.
2. | Disconnect the rheostat connector from the crash pad panel.
3. | Check for intensity. If the light intensity of the lamps changes smoothly without any flickering when the rheostat is turned, it can be assumed that the rheostat is normal.
FRONT FOG LAMP SWITCH
1. | Disconnect the negative (-) battery terminal.
2. | Detach the switch connector from the center facia panel.
3. | Operate the switch and check for continuity between the terminals with an ohmmeter.
MAP LAMP SWITCH