| TIBURON(GK) >2006 > G 2.0 DOHC > Restraint > Supplemental Restraint System Control Module (SRnodeM) > Side Impact Sensor (SIS)>Repair procedures |

REMOVAL
1. | Disconnect the negative battery cable and keep secure from battery.
Wait at least 3 minutes after disconnecting the battery cable before doing any further work.
2. | Remove the front seat.
3. | Remove the door scuff trim.
4. | Remove the guarter trim. After removing seat belt lower anchor bolt.
5. | Remove the floor carpet.
6. | Disconnect the SIS connector and remove the SIS.