| TIBURON(GK) >2006 > G 2.0 DOHC > Engine Electrical System > Starting System > Starter Relay>Repair procedures |

INSPECTION
1. | Remove the fuse box cover.
2. | Remove the starter relay(A).
3. | Inspect the relay continuity.
A. | Using an ohmmeter, check that there is continuity between terminals 2 and 4. If there is no continuity, replace the relay.
B. | Check that there is no continuity between terminals 1 and 5. If there is continuity, replace the relay.
4. | Inspect the relay operation.
A. | Apply battery positive voltage across terminals 2 and 4.
B. | Using an ohmmeter, check that there is continuity between terminals 1 and 5. If there is no continuity, replace the relay.
5. | Install the starter relay.
6. | Install the fuse box cover.