| TIBURON(GK) >2006 > G 2.0 DOHC > Restraint > General Information>Specifications |

SPECIFICATION
ITEM | SPECIFICATION
Driver Airbag (DAB) | Resistance(Ω) | 1.8~2.2Ω
Passenger Airbag(PAB) | Resistance(Ω) | 1.7~2.3Ω
Side Airbag(SAB) | Resistance(Ω) | 1.9~2.5Ω
Seat Belt Pretensioner (BPT) | Resistance(Ω) | 1.8~2.5Ω
Seat Belt Buckle Switch(BS) | Resistance(Ω) | Belted: 630~770Ω
Unbelted : 360~440Ω
TIGHTENING TORQUES
ITEM | kgf•m | N•m | lbf•ft
Driver Airbag (DAB) | 0.7~0.76 | 7~7.5 | 5.16~5.53
Passenger Airbag(PAB) | 0.7~1.12 | 7~11 | 5.16~5.53
Seat Belt Lower Anchor Bolt (BPT) | 4~5.5 | 39.23~53.94 | 5.16~5.53
SRSCM Mounting Bolt | 0.611~0.816 | 6~8 | 4.4~5.9
Side Impact Sensor (SIS) Mounting Bolt | 0.611~0.816 | 6~8 | 4.4~5.9