| TIBURON(GK) >2006 > G 2.7 DOHC > Clutch System > Clutch System > Clutch Pedal>Repair procedures |

REMOVAL
1. | Remove the cotter pin, washer and clevis pin.
2. | Remove the clutch pedal mounting bolt.
INSTALLATION
1. | Installation is the reverse of removal.
2. | Apply multi-purpose grease to the bushings.
3. | Apply multi-purpose grease to the clevis pin and washer.
4. | Install the push rod to the clutch pedal.
5. | Adjust the clutch pedal clevis pin play.
INSPECTION
1. | Check the clutch pedal shaft and bushing for wear.
2. | Check the clutch pedal for bending or distortion.
3. | Check the return spring for damage or deterioration.
4. | Check the clutch pedal pad for damage or wear.
IGNITION LOCK SWITCH INSPECTION