| TIBURON(GK) >2006 > G 2.7 DOHC > Brake System > ESP(Electronic Stability Program) System > Master Cylinder Pressure Sensor>Description and Operation |

DESCRIPTION
The pressure sensor(A) is connected to the master cylinder, when ESP is on operation, detecting the brake pressure in order to sense the user’s will to brake a vehicle. The pressure sensor(A) consists of two ceramic disks, one is fixed and the other movable, so that changes the distance of the two disks. (Max. measurable pressure is 200bar.) SPECIFICATIONS
Item | Specification | Remark
Supply voltage | 4.75V ~ 5.25V |
Supply current | less than 15mA |
Operating temperature | -40°C ~ 125°C |
Measurement pressure range | 0 ~ 200bar |
Max. pressure limit | 350bar |
Zero rate output | 0.5V |
Output range | 0.5 ~ 4.4V |
CIRCUIT DIAGRAM OUTPUT CHARACTERISTIC