| TIBURON(GK) >2006 > G 2.7 DOHC > Body Electrical System > Audio > Audio Unit>Repair procedures |

REMOVAL
1. | Disconnect the negative(-) battery terminal.
2. | Remove the center facia panel and disconnect the wire connectors.
3. | Remove the 4 screws holding the audio and multi-gauge unit then remove the audio assembly.
4. | Installation is the reverse of removal.
AUTO CD CHANGER
1. | Remove the right side quarter trim.
2. | Remove the auto CD changer from the right side quarter panel.
INSPECTION
TAPE HEAD AND CAPSTAN CLEANING
1. | To obtain optimum performance, clean the head, and capstan as often as necessary, depending on frequency of use and tape cleanness.
2. | To clean the tape head and capstan, use a cotton swab dipped in ordinary rubbing alcohol. Wipe the head and capstan.
AUDIO FAULT CODE
If you see any error indication in the display while using the CD or Tape mode, find the cause in the chart below.
INDICATION | CAUSE | SOLUTION
Er2 | CDP deck mechanical error (eject error, loading error) | After resetting the audio, push the eject button. If disc is not ejected, consult your hyundai dealer.
Er3 | Focus error Data read error | Make sure the disc is not scratched or damaged. Press the eject button and pull out the disc. Then insert a normal CD disc.
Er6 | Disc error | Check if the disc is inserted correctly in the CD player. Make sure the disc is not scratched or damaged.
Er8 | Tape deck error Tape eject error | After resetting the audio, push the eject button. If tape is not ejected, consult your hyundai dealer.
HHH | Temperature is too high | Fault code will reset automatically when the temperature returns to normal.
no CD | No disc in magazine No CD magazine in the auto change | Insert disc in magazine or insert CD magazine in the auto changer.
In order to reset the audio, pull out the audio fuse (10A) in the body control module after waiting at least 10 seconds, then insert the audio fuse.