| TIBURON(GK) >2006 > G 2.7 DOHC > Engine Electrical System > Cruise Control System>Repair procedures |

INSPECTION
CRUISE CONTROL SWITCH TEST
1. | Disconnect the battery negative cable, then disconnect the positive cable, and wait at least three minutes.
2. | Remove the driver's airbag (See page RT).
3. | Disconnect the control switch connector.
4. | Check the continuity between the terminals of the connector in each switch position according to the table.
A. | If there is continuity, and it matches the table, the switch is O.K.
B. | If there is no continuity, replace the control switch.
BRAKE SWITCH TEST
1. | Disconnect the connector from the brake switch.
2. | Remove the brake switch.
3. | Check for continuity between the terminals according to the table.
4. | If necessary, replace the switch or adjust the pedal height.
REPLACEMENT
CRUISE CONTROL UNIT AND CABLE
1. | Loosen the locknuts(A) and disconnect the actuator cable (B) from the throttle linkage(C).
2. | Disconnect the cruise control unit connector(D).
3. | Loosen the three mounting bolts(E), and remove the cruise control unit with the bracket(F).
4. | Loosen the locknuts(A) and disconnect the actuator cable(B) from the cruise control unit.
5. | Installation is the reverse of removal.
CRUISE CONTROL SWITCH REPLACEMENT
1. | Disconnect the battery negative cable, then disconnect the positive cable, and wait at least three minutes.
2. | Remove the driver's airbg (See page RT).
3. | Disconnect the control switch connector(A).
4. | Loosen the two mounting screws(B), and remove the cruise control switch.
5. | Installation is the reverse of removal.
6. | Connect the battery positive cable and negative cable to the battery.