| TIBURON(GK) >2006 > G 2.7 DOHC > Heating,Ventilation, Air Conditioning > Blower > Blower Unit>Repair procedures |

REMOVAL
1. | Disconnect the negative cable from the battery.
2. | Remove the crash pad (see BD group - crash pad).
3. | Disconnect the connectors(A) from the blower relay the blower motor, the blower resistor (or power transistor) and the fresh and recirculation actuator. Remove the self-tapping screws(B), the mounting nut(C), the mounting bolts(D) and the blower unit(E).
Make sure that there is no air leaking out of the blower and duct joints.
AIR FILTER REPLACEMENT
1. | Remove the mounting screws on the downside of the glove box.
2. | Open the glove box and remove the mounting screws on the upside of the glove box.
3. | Remove the filter cover.
4. | Replace the air filter with a new one.
5. | Installation is the reverse of the removal.