| TIBURON(GK) >2006 > G 2.7 DOHC > Body (Interior and Exterior) > Seat & Power Seat > rear seat>Repair procedures |

REMOVAL AND INSTALLATION
1. | Remove the mounting bolts and bracket from the rear seat back.
Tightening torque: 16.7~25.5 N•m (1.7~2.6 kgf•m, 12.3~18.8 lbf•ft)
2. | Remove the mounting bolts from the rear seat cushion.
Tightening torque: 16.7~25.5 N•m (1.7~2.6 kgf•m, 12.3~18.8 lbf•ft)
3. | Installation is the reverse of removal.