| TIBURON(GK) >2006 > G 2.7 DOHC > Driveshaft and axle > General Information>Specifications |

SPECIFICATIONS
Driveshaft
Joint type | 2.0L M/T | 2.0L A/T | 2.0L 6M/T | 2.7L
Outer | B.J. | B.J. | B.J. | B.J.
Inner | D.O.J. | T.J. | T.J. | T.J.
Maximum permissible joint angle
B.J. | 46° or more | 45.8° or more | 46° or more | 46.5° or more
D.O.J. | 22° or more |  |  |
T.J. |  | 23° or more | 23° or more | 23° or more
Hub end play mm(in.) | 0.008 (0.0003) or less
Wheel bearing starting torque Nm (kg•cm, lbf•ft) | 1.8 (18, 1.33) or less
B. J. : Birfield joint D.O.J. : Double offset joint T. J. : Tripod joint | M/T : 5 Speed Manual transaxle 6M/T : 6 Speed Manual transaxle A/T : Automatic transaxle
TIGHTENING TORQUE
| Nm | Kgf•cm | lbf•ft
Driveshaft nut 2.0L 2.7L | 200 ~ 260 200 ~ 280 | 2000 ~ 2600 2000 ~ 2800 | 148 ~ 192 148 ~ 207
Knuckle to strut assembly nut | 140 ~ 160 | 1400 ~ 1600 | 104 ~ 118
Lower arm ball joint to knuckle nut | 60 ~ 72 | 600 ~ 720 | 44 ~ 53
Tie rod end to knuckle | 24 ~ 34 | 240 ~ 340 | 18 ~ 25
Front brake caliper to knuckle | 69 ~ 85 | 690 ~ 850 | 51 ~ 63
Wheel nut | 90 ~ 110 | 900 ~ 1100 | 66 ~ 81
Rear hub bearing flange nut | 200 ~ 260 | 2000 ~ 2600 | 148 ~ 192
Rear brake to rear axle carrier mounting bolt | 65 ~ 75 | 650 ~ 750 | 48 ~ 56
Rear strut to carrier nut | 110 ~ 130 | 1100 ~ 1300 | 81 ~ 96
Trailing arm to rear axle carrier mounting nut | 100 ~ 120 | 1000 ~ 1200 | 74 ~ 88
Rear suspension arm to rear axle carrier mounting nut | 160 ~ 180 | 1600 ~ 1800 | 118 ~ 133
Replace self-locking nuts with new ones after removal.
LUBRICANTS
Items | Recommended | Quantity
Birfield joint + Double offset joint Type driveshaft (For 2.0L M/T)
Birfield joint boot grease | CENTOPLEX 278M/136K CASMOLY BJ ROLLUBE BJ Sunlight SW-2 | 115 ± 6gr.
Double offset joint boot greasE | AMBLYGON TA 10/2A CASMOLY DOJ DURALUBE DOJ Variant SD-R2 | 100 ± 6gr.
Birfield joint + Tripod joint Type driveshaft (For 2.0L 6M/T)
Birfield joint boot grease | CENTOPLEX 278M/136K CASMOLY BJ ROLLUBE BJ Sunlight SW-2 | 115 ± 6gr.
Tripod joint boot greas | KLK TJ 41-182 CASMOLY TJ ROLLUBE TJ Oneluber MK | 145 ± 6gr.
Birfield joint +Tripod joint Type driveshaft (For 2.0L A/T)
Birfield joint boot grease | CENTOPLEX 278M/136K CASMOLY BJ ROLLUBE BJ Sunlight SW-2 | 110 ± 6gr.
Tripod joint boot greas | KLK TJ 41-182 CASMOLY TJ ROLLUBE TJ Oneluber MK | 145 ± 6gr.
Birfield joint + Tripod joint Type driveshaft (For 2.7L)
Birfield joint boot grease | CENTOPLEX 278M/136K CASMOLY BJ ROLLUBE BJ Sunlight SW-2 | 135 ± 6gr.
Tripod joint boot grease | KLK TJ 41-182 CASMOLY TJ ROLLUBE TJ Oneluber MK | 145 ± 6gr.