| TIBURON(GK) >2006 > G 2.7 DOHC > Manual Transaxle System > Manual Transaxle System > Manual Transaxle>Repair procedures (MFA60) |

SERVICE ADJUSTMENT PROCEDURES
TRANSAXLE GEAR OIL LEVEL INSPECTION
1. | Remove oil filler plug and check level with finger.
2. | Oil level must be up to fill the hole, add oil until it runs over. Then reinstall plug.
3. | Replace the oil so that the transaxle gear oil is not dirty, and so that it is of a suitable viscosity.
REPLACEMENT OF TRANSAXLE GEAR OIL
1. | With the vehicle parked on a level surface, remove the drain plug and drain the transaxle oil.
2. | Replace the gasket with a new one and install the drain plug.
3. | Add new oil through the filler plug and, fill it to just below the plug opening.
Standard value Transaxle oil total capacity : MFA60 : 2.2 ± 0.1 liter
DRIVE SHAFT OIL SEAL REPLACEMENT
1. | Disconnect the drive shaft from the transaxle (Refer to "DS" group).
2. | Using a flat-tip screwdriver, remove the oil seal.
3. | Using the special tool (09431-2C000), tap the drive shaft oil seal into the transaxle.
4. | Apply a coating of gear oil to the oil seal.