| TIBURON(GK) >2007 > G 2.0 DOHC > Restraint > General Information>Description and Operation |

WARNING LAMP ACTIVATION
WARNING LAMP BEHAVIOR AFTER IGNITION ON As soon as the operating voltage is applied to the SRSCM ignition input, the SRSCM activates the warning lamp for a bulb check. The lamp shall turn on for 6 seconds during the initialization phase and be turned off afterward. However, in order to warn the driver, the warning lamp shall turn on for 6 seconds and off for one second then on continuously after the operating voltage is applied if any active fault exists.
1. | Active fault or historical fault counter is greater or equal to 10
2. | Normal or historical fault counter is less than 10
SRSCM INDEPENDENT WARNING LAMP ACTIVATION There are certain fault conditions in which the SRSCM cannot function and thus cannot control the operation of the standard warning lamp. In these cases, the standard warning lamp is directly activated by appropriate circuitry that operates independently of the SRSCM. These cases are:
1. | Loss of battery supply to the SRSCM : warning lamp turned on continuously.
2. | Loss of internal operating voltage : warning lamp turned on continuously.
3. | Loss of Microprocessor operation : warning lamp turned on continuously.
4. | SRSCM not connected : warning lamp turned on continuously through the shorting bar.
TELLTALE LAMP ACTIVATION The Telltale Lamp indicates the Passenger Airbag(PAB) enabled and disabled status based on occupant status of passenger seat. If the passenger seat is empty or occupied with child (or child seat), the Passenger Airbag is disabled and the Telltale Lamp is turned ON to inform the driver that the PAB is disabled. As soon as operating voltage is applied to the SRSCM ignition input, the SRSCM activates telltale lamp prove out. OCCUPANT STATUS INFORMATION AND TELLTALE
Occupant Status | Telltale Lamp | PAB
Empty | ON | Disabled
Child (Small Occupant) | ON | Disabled
Adult (Large Occupant) | OFF | Enabled
Indeterminate | ON | Disabled
After ignition on, telltale lamp will turn on for 4 seconds and turn off for 4 seconds during the initialization phase and be turned off afterward until receipt of first valid suppression message from OCS system.