| TIBURON(GK) >2007 > G 2.0 DOHC > Suspension System > Rear Suspension System > Trailing Arm>Repair procedures |

REMOVAL
1. | Detach the parking brake cable from the rear trailing arm bracket.
2. | After loosening the rear trailing arm mounting bolts, remove the trailing arm.
3. | Remove the rear suspension arm mounting bolt from the rear axle carrier.
4. | After supporting the center of the rear crossmember assembly with a jack, remove the rear crossmember mounting bolts to the body.
5. | Remove the rear crossmember and suspension arm.
REPLACEMENT
TRAILING ARM BUSHING
1. | Install the special tool (09551 - 25000) on the trailing arm.
2. | Remove the trailing arm bushing.
3. | Using the special tool (09551 - 25000), press-fit the rear trailing arm bushing.
Press-fit the bushing in the same way as shown in the illustration.
REAR SUSPENSION ARM BUSHING
1. | Install the special tools (09545-28100, 09552-25000) on the rear suspension arm.
2. | Remove the rear suspension bushing.
3. | Apply soap solution to the new bushing and the rear suspension arm.
4. | Using the special tool (09552-25000), press-fit the the bushing.