| TIBURON(GK) >2007 > G 2.0 DOHC > Engine Electrical System > Starting System > Starter>Repair procedures |

REMOVAL
1. | Disconnect the battery negative cable.
2. | Remove the starter cover.
3. | Disconnect the starter cable(A) from the B terminal(B) on the solenoid(C), then disconnect the connecto(D) from the S terminal(E).
4. | Remove the 2 bolts holding the starter, then remove the starter.
5. | Installation is the reverse of removal.
6. | Connect the battery negative cable to the battery.