| TIBURON(GK) >2007 > G 2.0 DOHC > Suspension System > General Information>Specifications |

SPECIFICATIONS
SERVICE STANDARD TIGHTENING TORQUE
Items | Nm | kgf•cm | lbf•ft
Wheel nut | 90~110 | 900~1100 | 67~82
Driveshaft nut 2.0L 2.7L | 200~260 200~280 | 2000~2600 2000~2800 | 148~192 148~207
Front strut upper installation nut | 45~60 | 450~600 | 33~44
Front strut assembly to knuckle | 140~160 | 1400~1600 | 104~118
Front strut mounting self-locking nut | 50~70 | 500~700 | 37~51
Lower arm ball joint to knuckle | 60~72 | 600~720 | 43~52
Lower arm bushing (A) mounting bolt | 130~150 | 1300~1500 | 96~111
Lower arm bushing (G) mounting bolt | 130~150 | 1300~1500 | 96~111
Stabilizer bar bracket mounting bolt | 30~45 | 300~450 | 22~33
Tie rod end ball joint to knuckle | 24~34 | 240~340 | 18~25
Tie rod end lock nut | 50~55 | 500~550 | 37~41
Stabilizer link nut | 35~45 | 350~450 | 26~33
Rear strut upper mounting nut | 30~40 | 300~400 | 22~30
Rear strut lower mounting nut | 110~130 | 1100~1300 | 81~96
Rear strut mounting self locking nut | 40~60 | 400~600 | 30~44
Rear stabilizer link to stabilizer bar | 35~45 | 350~450 | 26~33
Rear stabilizer bar bracket bolt | 17~26 | 170~260 | 13~19
Rear suspension arm tie rod nut | 50~60 | 500~600 | 37~43
Rear suspension arm (A,B) mounting bolt | 160~180 | 1600~1800 | 118~133
Rear cross member mounting bolt | 100~120 | 1000~1200 | 74~88
Trailing arm to bracket nut | 40~50 | 400~500 | 30~37
Trailing arm bracket to body frame | 40~50 | 400~500 | 30~37
Trailing arm mounting | 100~120 | 1000~1200 | 74~88
Replace the self-locking nuts with new ones after removal.
LUBRICANTS
Item | Recommended lubricant | Quantity
In ball joint of lower arm | Variant R-2 grease or poly lub gly 801K | As required