| TIBURON(GK) >2007 > G 2.0 DOHC > Heating,Ventilation, Air Conditioning > Blower > Control Panel>Description and Operation |

DESCRIPTION
1. | BLOWER SWITCH The blower switch controls the blowing level of the air conditioning system by controlling blower motor speed. The switch has an electrical circuit containing a resister that will regulate blower motor input voltage to control the motor speed.
2. | MODE SWITCH The mode switch controls air conditioning system discharge location. The switch contains an electrical circuit to control an actuator that is connected to the mode door for discharge control.
3. | TEMPERATURE SWITCH The temperature switch controls the temperature door position that will be used to regulate the air conditioning system's discharge air temperature. The switch includes a rack & pinion and a cable.
4. | INTAKE SWITCH The intake switch controls the intake door used to regulate the intake air flow of the air conditioning system. The switch contains an electrical circuit used to control the actuator that is connected to the intake door.
5. | AIR CONDITIONING SWITCH The air conditioning switch controls the on/off position of the air conditioning system compressor. The switch contains an electrical circuit that will switch on/off the power supply to the relay that is connected to the compressor.
6. | REAR DEFOGGER SWITCH The rear defogger switch is used to defog the rear glass. Switching the switch on, ETACS will output a signal to operate the rear glass heat wire.