| TIBURON(GK) >2007 > G 2.0 DOHC > Heating,Ventilation, Air Conditioning > Blower > Blower Motor>Description and Operation |

DESCRIPTION
Moter : Magnet Ø70
Item | Speccifications
Type | DC ferrite | 20°C or 68°F
Rated voltage | DC 12 volts
No load speed | Min. 3300rpm
No load current | Max. 3.0A
Rated load | 5.0kgf•cm
Speed in rated load | 2900 ± 250rpm
Current in rated load | Continuous
Insulation resistance | Min. 1MΩ
Rotation direction viewed from output (Mtr. shaft) | CCW
Operation temp. range | -30° ~ +80°