| TIBURON(GK) >2007 > G 2.0 DOHC > Body Electrical System > Rear Wiper/Washer > Rear Wiper Motor>Repair procedures |

REMOVAL
1. | Remove the upper and side trim from the tailgate frame.
2. | Remove the tailgate trim panel after removing 4 screws.
3. | Remove the rear wiper arm after removing a nut.
Tightening torque 14~17 Nm (140~170 kg•cm, 10.3~12.5 lb•ft)
4. | Remove the hexagonal nut after removing pivot cover.
Tightening torque 14~17 Nm (140~170 kg•cm, 10.3~12.5 lb•ft)
5. | Remove the rear wiper motor after removing 3 bolts, and disconnect the motor's connector.
INSTALLATION
1. | Installation is the reverse of removal.
2. | Set the washer nozzle on the specified spray position.
INSPECTION
1. | Remove the connector from the rear wiper motor.
2. | Connect battery positive (+) and negative (-) cables to terminals 3 and 4 respectively.
3. | Check that the motor operates normally. Replace the motor if it operates abnormally.