| TIBURON(GK) >2007 > G 2.0 DOHC > Body Electrical System > Fuses And Relays > Relay Box (Engine Compartment)>Repair procedures |

INSPECTION
1. | Check for a blown fusible link with an ohmmeter.
2. | If a fusible link burns out, there is a short or some other problem in the circuit. Carefully determine the cause and correct it before replacingthe fusible link.
The fusible link will burn out within 15 seconds if a higher than specified current flows through the circuit.