| TIBURON(GK) >2007 > G 2.0 DOHC > Restraint > Seat Belt Pretensioner > Seat Belt Retractor Pretensioner (BPT)>Repair procedures |

REMOVAL
1. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.
2. | Loosen the sliding bar mounting bolts.
3. | Remove the following parts. (Refer to BD group)
A. | Door scuff trim, Quarter trim
4. | Remove the upper anchor bolt.
5. | Loosen the Seat Belt Pretensioner mounting bolt and remove the Seat Belt Pretensioner.
6. | Disconnect the Seat Belt Pretensioner connector.
INSTALLATION
1. | Remove ignition key from the vehicle.
2. | Disconnect the negative (-) cable from battery and wait for at least three minutes.
3. | Connect the Seat Belt Pretensioner connector to the SRS main harness connector.
4. | Install the Seat Belt Pretensioner (BPT) with bolt.
5. | Install the upper anchor bolts.
Tightening Torque (Seat Belt Anchor Bolt) : 4.0 ~ 5.5 kgf.m (39.2 ~ 53.9 Nm, 28.9 ~ 39.8 lb.ft)
6. | Install the following parts (Refer to BD group).
A. | Quarter trim, Door scuff trim
7. | Install the sliding bar mounting bolts.
8. | Reconnect the negative battery cable.
9. | After installing the Seat Belt Pretensioner (BPT), confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.