| TIBURON(GK) >2007 > G 2.0 DOHC > Brake System > Brake System > Brake Pedal>Repair procedures |

REMOVAL
1. | Remove the stop lamp switch.
2. | Remove the split pin and clevis pin.
3. | Remove the flange nuts of the brake mounting bracket.
4. | Remove the brake pedal assembly.
INSTALLATION
1. | Installation is the reverse of removal.
Be sure to install the split pin on the operating rod clevis pin.
2. | Install the brake pedal assembly and tighten the flange nuts (booster mounting nuts) and bolt.
Tightening torque: 13~16 Nm (130~160 kgf•cm, 6~9 lbf•ft)
3. | Adjust the brake pedal height and free play.
4. | Install the stop lamp switch.
INSPECTION
1. | Check the bushing for wear.
2. | Check the brake pedal for distortion.
3. | Check the brake pedal return spring for damage.
4. | Check the stop lamp switch.
(1) | With an ohmmeter connected to the stop lamp switch terminals, check for continuity.
(2) | If there is no continuity when the plunger is depressed and there is continuity when the plunger is released, the stop lamp switch is normal.