| TIBURON(GK) >2007 > G 2.0 DOHC > Engine Mechanical System > Intake And Exhaust System > Front Exhsust Pipe>Repair procedures |

REMOVAL
1. | Remove the front muffler(A).
Tighening torque 29.4 ~ 39.2N.m(3.0 ~ 4.0kgf.m, 21.7 ~ 28.9lb-ft)
2. | Remove the catalytic converter(A).
Tighening torque 29.4 ~ 39.2N.m(3.0 ~ 4.0kgf.m, 21.7 ~ 28.9lb-ft)
3. | Remove the center muffler(A).
Tighening torque 29.4 ~ 39.2N.m(3.0 ~ 4.0kgf.m, 21.7 ~ 28.9lb-ft)
4. | Remove the main muffler(A).
Tighening torque 29.4 ~ 39.2N.m(3.0 ~ 4.0kgf.m, 21.7 ~ 28.9lb-ft)