| TIBURON(GK) >2007 > G 2.0 DOHC > Heating,Ventilation, Air Conditioning > Air conditioning System > Ambient sensor>Description and Operation |

DESCRIPTION
1. | The air temperature sensor, located at the front of the engine radiator, detects ambient air temperature. It is a negative type thermistor; resistance will increase with lower temperatures, and decrease with higher temperatures.
2. | The sensor output will be used for discharge temperature sensor, sensor fail-safe, temperature regulation door control, blower motor level control, mix mode control and in-car humidity control.
A. | R25°C : 30KΩ ± 3%
B. | B(0/25) : 3754K ± 2%
C. | Operation Temp. range : -30°C ~ 80°C