| TIBURON(GK) >2007 > G 2.0 DOHC > Engine Mechanical System > Intake And Exhaust System > Intake Manifold>Repair procedures |

REMOVAL
1. | Remove the engine cover.
2. | Disconnect the TPS connector(A) and ISA connector(B).
3. | Remove the PCV hose(A) and breather hose(B).
4. | Remove the accelerator cable by loosening the locknut, then slip the cable end out of the throttle linkage.
5. | Remove the delivery pipe(A).
6. | Remove the water hoses(A), PCSV(B), and brake vacuum hose(C).
7. | Remove the intake manifold stay(A).
8. | Remove the intake manifold.
9. | To install, reverse the removal procedure with new gasket.