| TIBURON(GK) >2007 > G 2.7 DOHC > Brake System > ABS(Anti-Lock Brake System) > Front Wheel Speed Sensor>Repair procedures |

REMOVAL
FRONT WHEEL SPEED SENSOR
1. | Remove the front wheel speed sensor mounting bolt.
2. | Remove the front wheel speed sensor after disconnecting the wheel speed sensor connector.
REAR WHEEL SPEED SENSOR
1. | Remove the rear wheel speed sensor mounting bolt.
2. | Remove the luggage trim and disconnect the wire connector from the rear wheel speed sensor.
INSPECTION
1. | Measure the output voltage between the teminal of the wheel speed sensor and the body ground.
In order to protect the wheel speed sensor, when measuring output voltage, a 100Ω resister must be used as shown.
1. | Compare the change of the output voltage of the wheel speed sensor to the normal change of the output voltage as shown below.
• | V_low : 590mV ~ 840mV
• | V_high : 1.18V ~ 1.68V
• | Frequency range : 1~2,000Hz