| TIBURON(GK) >2007 > G 2.7 DOHC > Body (Interior and Exterior) > Exterior > hood>Repair procedures |

ADJUSTMENT
Hood Hinge
1. | Loosen the hood hinge mounting bolt.
2. | Adjust the longitudinal and lateral positions of the hood by utilizing the holes in the hinge.
3. | Adjust front edge of hood in vertical direction by adjusting the hood stop and adjusting bumpers.
Hood Latch
1. | Loosen the hood lock mounting bolts.
2. | Adjust the alignment of the hood latch by adjusting the vertical and lateral position of the lock and by adjusting the height of the hood.