| TIBURON(GK) >2007 > G 2.7 DOHC > Restraint > Supplemental Restraint System Control Module (SRnodeM) > SRS Control Module (SRnodeM)>Repair procedures |

REMOVAL
1. | Remove ignition key from the vehicle.
2. | Disconnect the negative (-) cable from battery and wait for at least three minutes.
3. | Disconnect the DAB, PAB, SAB, and BPT connectors.
4. | Remove the floor console. (Refer to BD group)
5. | Disconnect the SRSCM harness connector from the SRSCM.
6. | Remove the SRSCM mounting nuts (3EA) from the SRSCM, then remove the SRSCM.
INSTALLATION
1. | Remove ignition key from the vehicle.
2. | Disconnect the negative (-) cable from battery and wait for at least three minutes.
3. | Install the SRSCM with the SRSCM mounting nuts.
Tightening Torque (SRSCM Mounting Bolt) : 0.7 ~ 0.9 kgf.m (7 ~ 9 Nm, 5.2 ~ 6.6 lb.ft)
4. | Connect the SRSCM harness connector.
5. | Install the floor console. (Refer to BD group)
6. | Connect the DAB, PAB, SAB and BPT connectors.
7. | Reconnect the battery negative cable.
8. | After installing the SRSCM, confirm proper system operation:
A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.