| TIBURON(GK) >2007 > G 2.7 DOHC > Body (Interior and Exterior) > Bumper > rear bumper>Repair procedures |

REMOVAL AND INSTALLATION
1. | Loosen the trunk trim mounting screws and remove the trunk trim .
2. | Loosen the rear bumper cover mounting screw from the rear wheel house.
3. | Remove the rear combination lamp. Disconnect the combination lamp connector.
4. | Loosen the rear bumper mounting bolts and screws, then rear bumper (A).
5. | Installation is the reverse of removal.