| TIBURON(GK) >2007 > G 2.7 DOHC > Engine Mechanical System > Intake And Exhaust System > Exhaust Manifold>Repair procedures |

REMOVAL
1. | Remove the under cover.
2. | Remove the front muffler(A).
3. | Disconnect the oxygen sensor connector.
4. | Remove the heat protector(A).
5. | Remove the exhaust manifold(A) and gasket(B).
INSTALLATION
1. | Install the exhaust manifold(A) and gasket(B).
Tightening torque 24.5 ~ 29.4Nm (2.5 ~ 3.0kgf.m, 18.1 ~ 21.7lb-ft)
2. | Install the heat protector(A).
Tightening torque 16.7 ~ 21.6Nm (1.7 ~ 2.2kgf.m, 12.3 ~ 15.9lb-ft)
3. | Connect the oxygen sensor connector.
4. | Install the front muffler(A).
Tightening torque 29.4 ~ 39.2Nm (3.0 ~ 4.0kgf.m, 21.7 ~ 28.9lb-ft)
5. | Install the under cover.