| TIBURON(GK) >2007 > G 2.7 DOHC > Suspension System > Tire Pressure Monitoring System > TPMS Receiver>Repair procedures |

REPLACEMENT
When the receiver first arrives for replacement:
1) | It will be in Virgin State.
2) | It will not be configured for any specific platform.
3) | It will not have any sensor ID's memorized.
• | It is important to make sure that the correct receiver is used to replace the faulty part i.e. it must be Low Line (PN 95800-2E500) and not High Line (PN 95800-26000) in order to have the correct inflation warning thresholds set.
• | Receiver software version must be 8.4 or higher. (Receiver software can be checked with hand tool.)
1. | Disconnect vehicle battery.
2. | Remove faulty part and fit bracket assembly to new part.
3. | Secure new part to vehicle and fit connector.
4. | Re-connect battery and turn Ignition on.
5. | Check that DTC flash rate matches Virgin State indication (see SS- ).
6. | Connect 'TPMS exciter' to the diagnostic connector.
7. | Write vehicle name to receiver. receiver will now automatically update monitoring parameters.
8. | Read sensor's ids with the 'TPMS exciter'. (Refer to 'SENSOR INITIATING PROCEDURE')
9. | Register sensor's ids to receiver.
10. | Register VIN number of the vehicle.(17 digits)
11. | Change receiver state from Virgin to Normal.
12. | Disconnect diagnostic link.
13. | Turn ignition off for approximately 10 seconds then turn it back on and check that Normal State is now indicated (see SS- ).