| TIBURON(GK) >2007 > G 2.7 DOHC > Brake System > ESP(Electronic Stability Program) System > Yaw-rate and Lateral G Sensor>Description and Operation |

DESCRIPTION
1. | The yaw-rate & lateral G sensor is applied for the ESC system.
2. | The yaw-rate is the angular velocity, when a vehicle turns a corner, and the lateral G is the acceleration to move a vehicle out of the way when cornering.
specifications
ITEM | SPECIFICATION | REMARK
Operating voltage | 4.75 ~ 5.25V |
Current consumption | less than 65mA |
Output voltage range | 0.5 ~4.5V |
Operating temperature | -40 ~85°C |
Yaw-rate sensor | Measurement range | -75 ~ +75°/sec |
Output voltage range | 0.5 ~ 4.5V |
Sensitivity | 26.67mV(°/sec.) |
Zero rate output | 2.5V |
Frequency response | 18~22Hz |
Lateral G. sensor | Measurement range | -1.5 ~ +1.5g |
Output voltage range | 0.5 ~ 4.5 V |
Sensitivity | 0.136V/g |
Zero rate output | 2.5V |
Frequency response | 50Hz |
output characteristic external diagram